** Generated by Mecway 16.0
*NODE
*ELEMENT,TYPE=B32
*ELEMENT,TYPE=B31
*NSET,NSET=pinned_support_nodes
*NSET,NSET=pinned_support_nodes(2)
*NSET,NSET=node_rotation_nodes
*NSET,NSET=force_nodes
*ELSET,ELSET=Reference
*ELSET,ELSET=Eall
*ELSET,ELSET=Lower_Flange
*ELSET,ELSET=Upper_Flange
*ELSET,ELSET=Web
*ELSET,ELSET=1
*ELSET,ELSET=2
*ELSET,ELSET=3
*ELSET,ELSET=4
*SURFACE,NAME=Face_Selection
20,S1
20,S2
20,S3
20,S5
19,S1
19,S2
19,S3
19,S5
18,S1
18,S2
18,S3
18,S5
17,S1
17,S2
17,S3
17,S5
16,S1
16,S2
16,S3
16,S5
15,S1
15,S2
15,S3
15,S5
14,S1
14,S2
14,S3
14,S5
13,S1
13,S2
13,S3
13,S5
*MATERIAL,NAME=Flange_82_x_7.4
*ELASTIC,TYPE=ISOTROPIC
210000000000,0
*DENSITY
7850
*MATERIAL,NAME=Web_145.2_x_5
*ELASTIC,TYPE=ISOTROPIC
210000000000,0
*DENSITY
7850
*MATERIAL,NAME=Material
*ELASTIC,TYPE=ISOTROPIC
1000000000,0
*BOUNDARY
1,4,,0
2,4,,0
3,4,,0
4,4,,0
5,4,,0
6,4,,0
7,4,,0
8,4,,0
*BOUNDARY
1,1,,0
1,2,,0
1,3,,0
*BOUNDARY
2,1,,0
2,2,,0
2,3,,0
*BEAM SECTION,ELSET=Lower_Flange,MATERIAL=Flange_82_x_7.4,SECTION=RECT,OFFSET2=10.3108
0.082,0.0074
0,1,0
*BEAM SECTION,ELSET=Upper_Flange,MATERIAL=Flange_82_x_7.4,SECTION=RECT,OFFSET2=-10.3108
0.082,0.0074
0,1,0
*BEAM SECTION,ELSET=Web,MATERIAL=Web_145.2_x_5,SECTION=RECT
0.1452,0.005
0,0,1
*BEAM SECTION,ELSET=Reference,MATERIAL=Material,SECTION=RECT
0.001,0.001
1,0,0
*STEP
*STATIC
*CLOAD
3,3,-10000
*NODE FILE,GLOBAL=YES
U
*EL FILE
S
*END STEP