M16 (16mm hex head bolt diameter), 2mm coarse pitch, 50mm full thread, Grade 4.6
M22 WASHER
M16 WASHER
M16 NUT

You can use the lowest grade parts, since the aluminum plate will get crushed by anything higher.
This occurs because; lowering the part grade, lowers the proof load and torque.
