**
**   Structure: cantilever beam.
**   Test objective: user beam element U1
**
*NODE, NSET=Nall
*ELEMENT, TYPE=U1, ELSET=Eall
*USER ELEMENT,TYPE=U1,NODES=2,INTEGRATION POINTS=2,MAXDOF=6
*BOUNDARY
1,1,6
*MATERIAL,NAME=EL
*ELASTIC
1.e7,.3
*BEAM SECTION,ELSET=Eall,MATERIAL=EL,SECTION=GENERAL
0.0625,3.2552e-4,0.,3.2552e-4,0.8333
0.,1.,0.
*STEP
*STATIC
*CLOAD
2,2,1.
*NODE PRINT,NSET=Nall
U
*EL PRINT,ELSET=Eall
S
*END STEP